(footprint "SP1 BoardConnector"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "J*"
		(at 0 -4.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "917a9844-9f3a-4c94-80e8-8d354a4083a8")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "SP1 BoardConnector"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "2c5be931-9722-41ff-9fd9-0c6278ebec77")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "d81ac225-7558-4cfe-88bf-1696c7a12cd4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "f01d2e45-e29f-4513-a1a9-6b2973a1d3f4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_line
		(start 0.6 -3.2)
		(end 0.6 -1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "3aa70938-586c-4a3e-a93d-02a45af703e9")
	)
	(fp_line
		(start 0.6 -3.2)
		(end 14.4 -3.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "34b53d18-e03e-4fbc-bf7a-c3cb36e989ef")
	)
	(fp_line
		(start 0.6 -1.8)
		(end 14.4 -1.8)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "d865b53d-ba89-433e-9e88-6e1c8c56a37b")
	)
	(fp_line
		(start 14.4 -1.8)
		(end 14.4 -3.2)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "Edge.Cuts")
		(uuid "8b4493d1-c2b9-4b50-944a-c37e23935916")
	)
	(fp_line
		(start 0 -5)
		(end 0 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "e510258b-3779-4875-b420-1117887d3fe3")
	)
	(fp_line
		(start 0 -5)
		(end 15 -5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "71181587-a5e9-4b16-8773-da3d6030b578")
	)
	(fp_line
		(start 0 0)
		(end 15 0)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "ed6d23eb-65c5-4aee-bf06-6857d2f9baeb")
	)
	(fp_line
		(start 15 0)
		(end 15 -5)
		(stroke
			(width 0.05)
			(type default)
		)
		(layer "F.CrtYd")
		(uuid "20bf647a-5a63-447c-a674-2fe707034fb5")
	)
	(fp_text user "SP1 Board Connector"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "5049463d-dac6-4437-b3a8-a1b5edb5a60d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 13 -1.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "e971ccee-5fc7-4f69-ba9a-824295cdcea2")
	)
	(pad "1" smd rect
		(at 13 -0.8)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "68ca1828-1ce0-4ac2-a34f-4e525800f427")
	)
	(pad "2" smd rect
		(at 12 -4.2)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(uuid "b399b7b5-f95d-42af-b6ad-b8005e0e220a")
	)
	(pad "2" thru_hole circle
		(at 12 -3.2)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(uuid "c081903f-06d0-49e6-8b65-f59af44fab20")
	)
	(pad "3" thru_hole circle
		(at 11 -1.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "3b00d3b0-db71-4798-bfe8-f13c5a2fcfaa")
	)
	(pad "3" smd rect
		(at 11 -0.8)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c116c3ec-fbb3-41c8-a463-03c5730eee75")
	)
	(pad "4" smd rect
		(at 10 -4.2)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "f3b3df72-cf3c-4b3e-aa53-f60eafad05a8")
	)
	(pad "4" thru_hole circle
		(at 10 -3.2)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "a8162bd4-0568-4e63-8589-609e77851082")
	)
	(pad "5" thru_hole circle
		(at 9 -1.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "202faad8-5882-4212-9e6a-b6f9c3e66930")
	)
	(pad "5" smd rect
		(at 9 -0.8)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "87526c8b-1cd3-41f0-999c-e216a3f57cdb")
	)
	(pad "6" smd rect
		(at 8 -4.2)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "c56be59a-42d4-48a5-b264-1978d4c0747b")
	)
	(pad "6" thru_hole circle
		(at 8 -3.2)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "339533d2-b572-4150-9b16-22f4efdd8ffb")
	)
	(pad "7" thru_hole circle
		(at 7 -1.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "c6e88173-b541-4899-9265-73ec016138a9")
	)
	(pad "7" smd rect
		(at 7 -0.8)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "4fb36b6b-3c00-4e69-914f-a1a7225dc3ff")
	)
	(pad "8" smd rect
		(at 6 -4.2)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "65548375-2618-420f-b3ad-5c2263234b88")
	)
	(pad "8" thru_hole circle
		(at 6 -3.2)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "6fb12c8a-c11a-4e3e-9185-89d6876affb9")
	)
	(pad "9" thru_hole circle
		(at 5 -1.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "70d28bcf-0b92-47b9-96a8-f57184b8cdf3")
	)
	(pad "9" smd rect
		(at 5 -0.8)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "5133a63d-f4e8-43e5-ad45-2358f3ff29e2")
	)
	(pad "10" smd rect
		(at 4 -4.2)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(uuid "13d69f16-7af3-499e-81b5-b43f738487e5")
	)
	(pad "10" thru_hole circle
		(at 4 -3.2)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(thermal_bridge_angle 90)
		(uuid "0e39b6c5-911d-4e5e-ab8b-f026bf957e16")
	)
	(pad "11" thru_hole circle
		(at 3 -1.8)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(uuid "e1c2f8b8-87e1-4dad-8d12-a793452e85f2")
	)
	(pad "11" smd rect
		(at 3 -0.8)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(uuid "2aa85fd9-17bc-4938-9c98-fa1edc53590c")
	)
	(pad "12" smd rect
		(at 2 -4.2)
		(size 1.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(uuid "edc0cec0-2ddb-44d7-8cae-959b588c39d2")
	)
	(pad "12" thru_hole circle
		(at 2 -3.2)
		(size 1.5 1.5)
		(drill 1)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(uuid "4bb3c4fe-a697-41c9-a6b4-979c545a78c0")
	)
	(embedded_fonts no)
)
