
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
	(symbol "PUSB3AB6Z_ES"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(in_pos_files yes)
		(duplicate_pin_numbers_are_jumpers no)
		(property "Reference" "D"
			(at -10.16 10.16 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Value" "PUSB3AB6Z(ES)"
			(at -10.16 -10.16 0)
			(show_name no)
			(do_not_autoplace no)
			(effects
				(font
					(size 1.27 1.27)
				)
				(justify left bottom)
			)
		)
		(property "Footprint" "hardware:SON50P110X213X50-7"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/PUSB3AB6.pdf"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "6-channel 3.3V 0.15pF ultra-low-cap TVS array (Nexperia PUSB3AB6Z, ElecSuper 2nd source), DFN2111-7"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "MF" "ElecSuper"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "LCSC" "C49383400"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "ki_keywords" "TVS ESD array diode protection USB3 low capacitance"
			(at 0 0 0)
			(show_name no)
			(do_not_autoplace no)
			(hide yes)
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(symbol "PUSB3AB6Z_ES_0_1"
			(rectangle
				(start -5.08 8.89)
				(end 5.08 -8.89)
				(stroke
					(width 0.254)
					(type default)
				)
				(fill
					(type background)
				)
			)
		)
		(symbol "PUSB3AB6Z_ES_1_1"
			(pin passive line
				(at -10.16 6.35 0)
				(length 5.08)
				(name "CH1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "1"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin power_in line
				(at 0 -13.97 90)
				(length 5.08)
				(name "GND"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 3.81 0)
				(length 5.08)
				(name "CH2"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 1.27 0)
				(length 5.08)
				(name "CH3"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -1.27 0)
				(length 5.08)
				(name "CH4"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -3.81 0)
				(length 5.08)
				(name "CH5"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
			(pin passive line
				(at -10.16 -6.35 0)
				(length 5.08)
				(name "CH6"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
				(number "7"
					(effects
						(font
							(size 1.016 1.016)
						)
					)
				)
			)
		)
	)
)
