(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(J1-Ground-Pad11)")
	(net 2 "Net-(J2-3.3V)")
	(net 3 "Net-(J1-INT)")
	(net 4 "Net-(J1-12V)")
	(net 5 "Net-(J1-ExtIn)")
	(net 6 "Net-(J1-DI)")
	(net 7 "Net-(J1-Ground(Shield))")
	(net 8 "Net-(J1-CLK)")
	(net 9 "Net-(J1-Ground-Pad12)")
	(net 10 "Net-(J1-DO)")
	(net 11 "Net-(J1-CS)")
	(net 12 "Net-(J3-3.3V)")
	(footprint "Connector_FFC-FPC:JUSHUO_AFA07-S08FCA-00_1x8-1MP_P1.0mm_Horizontal"
		(layer "F.Cu")
		(uuid "094c15a6-4733-44d9-ada0-eaf3abcddd55")
		(at 224.15 136.205)
		(descr "JUSHUO FPC connector, 08 bottom-side contacts, 1.0mm pitch, 2.5mm height, SMT, https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_JUSHUO-AFA07-S04FCA-00_C262710.pdf")
		(tags "jushuo fpc")
		(property "Reference" "J3"
			(at 0 -5.48 0)
			(layer "F.SilkS")
			(uuid "5d2a42b7-d144-4023-b203-8cc7617dc560")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 5.68 0)
			(layer "F.Fab")
			(uuid "79e4b917-c068-4e9f-97d0-691e86119869")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "009ddd8b-3a73-4c29-b21d-a87c5a6bd58a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f0419484-0774-4f10-96ad-9c6562db8c4a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/294eee87-2b24-49ca-9367-623b8f90c5c4")
		(sheetname "/")
		(sheetfile "sp1_test_plug.kicad_sch")
		(attr smd)
		(fp_line
			(start -7.61 1.825)
			(end -7.26 0.325)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46eadf91-db1c-4a59-9fac-650221ba3a1b")
		)
		(fp_line
			(start -7.61 2.935)
			(end -7.61 1.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "26fa4492-c3b3-47b9-8489-4450c00db23d")
		)
		(fp_line
			(start 4.06 -2.585)
			(end 4.29 -2.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "48267fa7-7fae-495b-9f3a-5caa9f80d6f4")
		)
		(fp_line
			(start 7.26 0.325)
			(end 7.61 1.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "349356a9-3051-46da-b603-607a45dab402")
		)
		(fp_line
			(start 7.61 1.825)
			(end 7.61 2.935)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e91cdd3-c1f1-438f-9c5c-ea918631106f")
		)
		(fp_line
			(start 7.61 2.935)
			(end -7.61 2.935)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76cf38c1-d43c-4644-9053-d8e947cf4c4f")
		)
		(fp_poly
			(pts
				(xy -4.19 -3.405) (xy -4.52 -3.165) (xy -4.52 -3.645)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "7edfc595-e329-4210-8534-a1d96565d7c0")
		)
		(fp_line
			(start -8 -4.78)
			(end -8 4.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "86ae355d-0ed2-43b1-9673-b13b5b8455d3")
		)
		(fp_line
			(start -8 4.98)
			(end 8 4.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3a57f630-1886-4cb1-b0d0-8e402d39294d")
		)
		(fp_line
			(start 8 -4.78)
			(end -8 -4.78)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3bd9c07-3fe2-4398-b5c8-df23fa5158a9")
		)
		(fp_line
			(start 8 4.98)
			(end 8 -4.78)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "528d34fc-8967-41b9-a68c-3c33c3485fc8")
		)
		(fp_line
			(start -7.5 1.825)
			(end -7.15 0.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50759e17-cae4-4126-b499-7c9ed4b42aa7")
		)
		(fp_line
			(start -7.5 2.825)
			(end -7.5 1.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ca1d31fd-2bfd-49e2-a8c8-bd69843f6db1")
		)
		(fp_line
			(start -7.5 3.475)
			(end -6.525 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3c7533d3-4f42-4283-a9f9-f3156edff704")
		)
		(fp_line
			(start -7.5 4.475)
			(end -7.5 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "fc3fd87a-79f7-4e7d-99a4-fdcfd2581b35")
		)
		(fp_line
			(start -7.15 -0.675)
			(end -6.525 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3d62703c-f938-414d-8b30-085a78322060")
		)
		(fp_line
			(start -7.15 0.325)
			(end -7.15 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cccf09fd-478a-42a5-8a9f-9b2fc8159a5f")
		)
		(fp_line
			(start -6.525 -2.475)
			(end 6.525 -2.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ce7feeb5-bda8-4002-85b0-94d78ab4b326")
		)
		(fp_line
			(start -6.525 -0.675)
			(end -6.525 -2.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "45374cd4-760a-4739-bd74-4c8d13e3bae9")
		)
		(fp_line
			(start -6.525 3.475)
			(end -6.525 2.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "19bc967b-6b14-440b-99b1-edd39cc3b901")
		)
		(fp_line
			(start -4 -2.475)
			(end -3.5 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "baa0b5f8-016b-45ea-8593-c39f3a16c035")
		)
		(fp_line
			(start -3.5 -1.475)
			(end -3 -2.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1ec195e-8c57-4e62-b584-3df4a945f9a3")
		)
		(fp_line
			(start 6.525 -2.475)
			(end 6.525 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d704578d-cd5d-4942-8867-b2534504bbd9")
		)
		(fp_line
			(start 6.525 -0.675)
			(end 7.15 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "00c54830-fb61-4521-9792-e6dc6c0d3342")
		)
		(fp_line
			(start 6.525 2.825)
			(end 6.525 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2ac83406-4952-45b6-ba9f-8c895a925abd")
		)
		(fp_line
			(start 6.525 3.475)
			(end 7.5 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb48737e-a080-41e8-ab8c-52892aa73c79")
		)
		(fp_line
			(start 7.15 -0.675)
			(end 7.15 0.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "face3ba6-a636-4a19-a9bc-ed5a81e74f6f")
		)
		(fp_line
			(start 7.15 0.325)
			(end 7.5 1.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "9b93c205-4912-4b1f-a271-edd6994eaa17")
		)
		(fp_line
			(start 7.5 1.825)
			(end 7.5 2.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4e76a819-6ddc-4f3f-a921-a269d8bad224")
		)
		(fp_line
			(start 7.5 2.825)
			(end -7.5 2.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "615c4434-84ae-4e51-91eb-0eda66d55922")
		)
		(fp_line
			(start 7.5 3.475)
			(end 7.5 4.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62b7e43a-cb5b-4a8c-a63d-97c680c3f8fd")
		)
		(fp_line
			(start 7.5 4.475)
			(end -7.5 4.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7cceb5d7-0b28-4955-b884-b82a2ffbc96f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0.18 0)
			(layer "F.Fab")
			(uuid "b8763a66-8c63-402b-ab5b-dce391870037")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(J1-Ground(Shield))")
			(pinfunction "Shield")
			(pintype "power_out")
			(uuid "080c2f1a-5eeb-47a2-8475-d953462babff")
		)
		(pad "2" smd roundrect
			(at -2.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(J1-CLK)")
			(pinfunction "CLK")
			(pintype "output")
			(uuid "22973de8-a3b7-4cb7-9f0d-5a812fabc26d")
		)
		(pad "3" smd roundrect
			(at -1.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Ground-Pad12)")
			(pinfunction "GND")
			(pintype "power_out")
			(uuid "4285c46f-54ed-4fe8-a939-9e2aad343fdc")
		)
		(pad "4" smd roundrect
			(at -0.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J1-DO)")
			(pinfunction "DO")
			(pintype "output")
			(uuid "58fe090a-a0d9-46b7-b900-e04c63540d70")
		)
		(pad "5" smd roundrect
			(at 0.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J3-3.3V)")
			(pinfunction "3.3V")
			(pintype "power_out")
			(uuid "dcbd59a2-141b-4d53-a7bd-689a212b6383")
		)
		(pad "6" smd roundrect
			(at 1.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Ground-Pad12)")
			(pinfunction "GND")
			(pintype "power_out")
			(uuid "2311e56d-96fb-4525-a4b3-666311014549")
		)
		(pad "7" smd roundrect
			(at 2.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(J1-CS)")
			(pinfunction "CS")
			(pintype "output")
			(uuid "889ee080-7252-4e40-adca-8cb95796d2b4")
		)
		(pad "8" smd roundrect
			(at 3.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J1-Ground-Pad12)")
			(pinfunction "GND")
			(pintype "power_out")
			(uuid "e12262f3-f0e6-4443-b852-8ab0dc166793")
		)
		(pad "MP" smd roundrect
			(at -5.85 -1.205)
			(size 2.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.096154)
			(uuid "d2cbf631-bc7b-4555-88b3-9e37d35202f9")
		)
		(pad "MP" smd roundrect
			(at 5.85 -1.205)
			(size 2.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.096154)
			(uuid "e69021b7-6160-4764-a50f-5eddefc9e05f")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/JUSHUO_AFA07-S08FCA-00_1x8-1MP_P1.0mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:JUSHUO_AFA07-S08FCA-00_1x8-1MP_P1.0mm_Horizontal"
		(layer "F.Cu")
		(uuid "672c9c34-493b-41be-ab3e-134d28fb07c3")
		(at 224.15 125.395)
		(descr "JUSHUO FPC connector, 08 bottom-side contacts, 1.0mm pitch, 2.5mm height, SMT, https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_JUSHUO-AFA07-S04FCA-00_C262710.pdf")
		(tags "jushuo fpc")
		(property "Reference" "J2"
			(at 0 -5.48 0)
			(layer "F.SilkS")
			(uuid "179454ee-2283-4b27-b5bd-1d2391b82e9b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "~"
			(at 0 5.68 0)
			(layer "F.Fab")
			(uuid "8a99cda3-2531-4fbb-b925-43c7b0a4b6c0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0e7ef75b-1f23-4501-ba57-c4a60c648d69")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0cbf6e19-cb0b-442a-8e8e-a297047ce8d3")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(path "/e3bec88d-408c-4410-bf03-cee5171b4d71")
		(sheetname "/")
		(sheetfile "sp1_test_plug.kicad_sch")
		(attr smd)
		(fp_line
			(start -7.61 1.825)
			(end -7.26 0.325)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e5ad6d88-d0ee-4209-b41c-f3ae7c2981ee")
		)
		(fp_line
			(start -7.61 2.935)
			(end -7.61 1.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "97162ce8-456d-4da9-83af-30b9e2702d09")
		)
		(fp_line
			(start 4.06 -2.585)
			(end 4.29 -2.585)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a8c4d7f9-3481-4cd5-aaf6-3ae6b6bca5f3")
		)
		(fp_line
			(start 7.26 0.325)
			(end 7.61 1.825)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bab8c5f7-2424-4a35-bf62-38daef88932c")
		)
		(fp_line
			(start 7.61 1.825)
			(end 7.61 2.935)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0c85893c-409e-44d4-8ae8-c1eef1b9c25e")
		)
		(fp_line
			(start 7.61 2.935)
			(end -7.61 2.935)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4ca41856-0eb5-44d1-9dbf-408614d467ac")
		)
		(fp_poly
			(pts
				(xy -4.19 -3.405) (xy -4.52 -3.165) (xy -4.52 -3.645)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "48fec7fd-0c26-406c-9ffb-3ab123e3f283")
		)
		(fp_line
			(start -8 -4.78)
			(end -8 4.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ab0606e8-72f1-48d7-80f7-c1b9694df879")
		)
		(fp_line
			(start -8 4.98)
			(end 8 4.98)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5c94e065-a474-4778-87f9-33062aabac75")
		)
		(fp_line
			(start 8 -4.78)
			(end -8 -4.78)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc09b4f5-ac7f-4fe9-81d0-542ec3aaf392")
		)
		(fp_line
			(start 8 4.98)
			(end 8 -4.78)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15c99d9d-5596-429b-8aef-d851285bc843")
		)
		(fp_line
			(start -7.5 1.825)
			(end -7.15 0.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8d6866dd-723f-4461-9bee-4aa1dbd793d3")
		)
		(fp_line
			(start -7.5 2.825)
			(end -7.5 1.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62c282e0-d74b-4edc-981d-ee251bb7d781")
		)
		(fp_line
			(start -7.5 3.475)
			(end -6.525 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "471d4f75-0b12-4d39-b117-88045051fa8b")
		)
		(fp_line
			(start -7.5 4.475)
			(end -7.5 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "103c852e-14e3-43f2-9643-a14aa6d1f448")
		)
		(fp_line
			(start -7.15 -0.675)
			(end -6.525 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a95496b9-093c-4fdb-8761-8172f751a3d8")
		)
		(fp_line
			(start -7.15 0.325)
			(end -7.15 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2848b611-9ab3-45a3-8a37-e83b58b8b535")
		)
		(fp_line
			(start -6.525 -2.475)
			(end 6.525 -2.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "413f381a-b81d-4e85-994c-27af47c849f1")
		)
		(fp_line
			(start -6.525 -0.675)
			(end -6.525 -2.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "312fca1b-1d9b-4ba0-8928-8b901b8736ab")
		)
		(fp_line
			(start -6.525 3.475)
			(end -6.525 2.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8308e6de-e0ce-4c1d-8e43-edf4a93b5642")
		)
		(fp_line
			(start -4 -2.475)
			(end -3.5 -1.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5bd3ecc9-f393-45f0-a23f-72fa1fd1c0f1")
		)
		(fp_line
			(start -3.5 -1.475)
			(end -3 -2.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6d79835b-5ee0-4def-b29d-bee92211f3bf")
		)
		(fp_line
			(start 6.525 -2.475)
			(end 6.525 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "feb9f196-a605-40d7-874d-5f97f3b19f17")
		)
		(fp_line
			(start 6.525 -0.675)
			(end 7.15 -0.675)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0c7d156d-e59d-4f43-a5fc-38fe7088db1e")
		)
		(fp_line
			(start 6.525 2.825)
			(end 6.525 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5c772f0f-0860-4066-aa0b-519759da4636")
		)
		(fp_line
			(start 6.525 3.475)
			(end 7.5 3.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4925db26-4a6e-4020-ba99-26f380d77935")
		)
		(fp_line
			(start 7.15 -0.675)
			(end 7.15 0.325)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8010eb01-0336-4625-826b-e838e7bb854d")
		)
		(fp_line
			(start 7.15 0.325)
			(end 7.5 1.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0b4e9a25-1321-4632-b0f2-0b29fcba0de8")
		)
		(fp_line
			(start 7.5 1.825)
			(end 7.5 2.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3ce0ea2a-2be4-4df9-bbbf-64d265bd74ef")
		)
		(fp_line
			(start 7.5 2.825)
			(end -7.5 2.825)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6a0b0210-c26a-4745-9d72-6261f918947a")
		)
		(fp_line
			(start 7.5 3.475)
			(end 7.5 4.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "374f4103-8dbd-4a84-94ec-486a7dcd3181")
		)
		(fp_line
			(start 7.5 4.475)
			(end -7.5 4.475)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a6c82018-b23c-4455-bc51-e168dc4bdeba")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0.18 0)
			(layer "F.Fab")
			(uuid "19d115d2-2c32-4f89-a209-c0f4b97d81d9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "1" smd roundrect
			(at -3.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-ExtIn)")
			(pinfunction "ExtIn")
			(pintype "output")
			(uuid "b233ddc7-0584-4131-bf4d-f1eabc06f5be")
		)
		(pad "2" smd roundrect
			(at -2.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(J1-INT)")
			(pinfunction "Int")
			(pintype "output")
			(uuid "946a010f-5ce6-4c17-84c0-8577b518bed9")
		)
		(pad "3" smd roundrect
			(at -1.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-Ground-Pad11)")
			(pinfunction "GND")
			(pintype "power_out")
			(uuid "17fe7f86-29a4-488a-9f08-cf91ca41b936")
		)
		(pad "4" smd roundrect
			(at -0.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(J1-12V)")
			(pinfunction "12V")
			(pintype "power_out")
			(uuid "ad2c11ad-6b68-4dd0-81a1-ade7fe4f94f3")
		)
		(pad "5" smd roundrect
			(at 0.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(J2-3.3V)")
			(pinfunction "3.3V")
			(pintype "power_out")
			(uuid "21a56957-5154-4dea-8592-b6c54456fd6d")
		)
		(pad "6" smd roundrect
			(at 1.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-Ground-Pad11)")
			(pinfunction "GND")
			(pintype "power_out")
			(uuid "649603e0-95cd-4b1e-a635-fc40afc6ffa1")
		)
		(pad "7" smd roundrect
			(at 2.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J1-DI)")
			(pinfunction "DI")
			(pintype "output")
			(uuid "fb79afba-0a1a-4221-8b9f-581d224ca168")
		)
		(pad "8" smd roundrect
			(at 3.5 -3.375)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(J1-Ground-Pad11)")
			(pinfunction "GND")
			(pintype "power_out")
			(uuid "ffe72469-717f-429e-98c1-5fec5dd853a8")
		)
		(pad "MP" smd roundrect
			(at -5.85 -1.205)
			(size 2.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.096154)
			(uuid "1fe7e366-153b-4cab-896d-2b1ccd96981e")
		)
		(pad "MP" smd roundrect
			(at 5.85 -1.205)
			(size 2.6 3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.096154)
			(uuid "5bbad0a7-5c2e-486d-9add-1140c289f3f6")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/JUSHUO_AFA07-S08FCA-00_1x8-1MP_P1.0mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
)
