
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "HR961160C" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -10.16 25.908 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "HR961160C" (id 1) (at -10.16 -27.94 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "HR961160C:HANRUN_HR961160C" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "HanRun" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "15.63 mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "Package" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/HR961160C/HanRun/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "B" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/HR961160C/HanRun/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "HR961160C" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            1x1 Port Tab-UP Surface Mount RJ45 Connector with Magnetics Module and LED\nfor 10/100Base-TX NIC Applications.\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "HanRun" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "HR961160C_0_0"
      (rectangle (start -10.16 -25.4) (end 10.16 25.4)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin bidirectional line (at -15.24 10.16 0) (length 5.08)
        (name "CT_TD"
          (effects (font (size 1.016 1.016)))
        )
        (number "P5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 20.32 0) (length 5.08)
        (name "CT_RD"
          (effects (font (size 1.016 1.016)))
        )
        (number "P6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -15.24 -22.86 0) (length 5.08)
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -15.24 -22.86 0) (length 5.08) hide
        (name "SHIELD"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 17.78 0) (length 5.08)
        (name "RD+"
          (effects (font (size 1.016 1.016)))
        )
        (number "P7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 22.86 0) (length 5.08)
        (name "RD-"
          (effects (font (size 1.016 1.016)))
        )
        (number "P8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 7.62 0) (length 5.08)
        (name "TD+"
          (effects (font (size 1.016 1.016)))
        )
        (number "P3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -15.24 12.7 0) (length 5.08)
        (name "TD-"
          (effects (font (size 1.016 1.016)))
        )
        (number "P4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -15.24 2.54 0) (length 5.08)
        (name "YELLOW_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "P1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -15.24 0.0 0) (length 5.08)
        (name "YELLOW_K"
          (effects (font (size 1.016 1.016)))
        )
        (number "P2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -15.24 -5.08 0) (length 5.08)
        (name "GREEN_A"
          (effects (font (size 1.016 1.016)))
        )
        (number "P12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at -15.24 -7.62 0) (length 5.08)
        (name "GREEN_K"
          (effects (font (size 1.016 1.016)))
        )
        (number "P11"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -15.24 -17.78 0) (length 5.08)
        (name "CHS_GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "P10"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin no_connect line (at -15.24 -12.7 0) (length 5.08)
        (name "NC"
          (effects (font (size 1.016 1.016)))
        )
        (number "P9"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)